Suppose there are N nodes that use the slotted ALOHA protocol to contend for a channel. Among these nodes, node A has more data to transmit and has a transmission probability of while the other nodes’ transmission probability is .

Provide a formula for node A’s average throughput. What is the total efficiency of the protocol with these nodes?